-- Accepting DIAL from 172.27.28.126, formats = 0x4
    -- Executing [602@userauth:1] Dial("IAX2/iaxy-5", "SIP/tyril,30|t") in new stack
  == Using SIP RTP TOS bits 184
  == Using SIP RTP CoS mark 5
Audio is at 71.230.52.141 port 40072
Adding codec 0x4 (ulaw) to SDP
Adding codec 0x2 (gsm) to SDP
Adding codec 0x8 (alaw) to SDP
Adding codec 0x10 (g726aal2) to SDP
Adding codec 0x20 (adpcm) to SDP
Adding codec 0x40 (slin) to SDP
Adding codec 0x80 (lpc10) to SDP
Adding codec 0x400 (ilbc) to SDP
Adding codec 0x800 (g726) to SDP
Adding codec 0x1000 (g722) to SDP
Adding codec 0x8000 (slin16) to SDP
Adding non-codec 0x1 (telephone-event) to SDP
Reliably Transmitting (NAT) to 68.39.201.62:32958:
INVITE sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Contact: <sip:0000000000600@71.230.52.141:5066>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 INVITE
User-Agent: matrix.gs asterisk
Date: Tue, 29 Jan 2008 01:07:01 GMT
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces, timer
Content-Type: application/sdp
Content-Length: 506

v=0
o=root 520646963 520646963 IN IP4 71.230.52.141
s=session
c=IN IP4 71.230.52.141
t=0 0
m=audio 40072 RTP/AVP 0 3 8 112 5 10 7 97 111 9 101
a=rtpmap:0 PCMU/8000
a=rtpmap:3 GSM/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:112 AAL2-G726-32/8000
a=rtpmap:5 DVI4/8000
a=rtpmap:10 L16/8000
a=rtpmap:7 LPC/8000
a=rtpmap:97 iLBC/8000
a=fmtp:97 mode=30
a=rtpmap:111 G726-32/8000
a=rtpmap:9 G722/16000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-16
a=silenceSupp:off - - - -
a=ptime:20
a=sendrecv

---
    -- Called tyril
Retransmitting #1 (NAT) to 68.39.201.62:32958:
INVITE sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Contact: <sip:0000000000600@71.230.52.141:5066>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 INVITE
User-Agent: matrix.gs asterisk
Date: Tue, 29 Jan 2008 01:07:01 GMT
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces, timer
Content-Type: application/sdp
Content-Length: 506

v=0
o=root 520646963 520646963 IN IP4 71.230.52.141
s=session
c=IN IP4 71.230.52.141
t=0 0
m=audio 40072 RTP/AVP 0 3 8 112 5 10 7 97 111 9 101
a=rtpmap:0 PCMU/8000
a=rtpmap:3 GSM/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:112 AAL2-G726-32/8000
a=rtpmap:5 DVI4/8000
a=rtpmap:10 L16/8000
a=rtpmap:7 LPC/8000
a=rtpmap:97 iLBC/8000
a=fmtp:97 mode=30
a=rtpmap:111 G726-32/8000
a=rtpmap:9 G722/16000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-16
a=silenceSupp:off - - - -
a=ptime:20
a=sendrecv

---
Retransmitting #2 (NAT) to 68.39.201.62:32958:
INVITE sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Contact: <sip:0000000000600@71.230.52.141:5066>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 INVITE
User-Agent: matrix.gs asterisk
Date: Tue, 29 Jan 2008 01:07:01 GMT
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces, timer
Content-Type: application/sdp
Content-Length: 506

v=0
o=root 520646963 520646963 IN IP4 71.230.52.141
s=session
c=IN IP4 71.230.52.141
t=0 0
m=audio 40072 RTP/AVP 0 3 8 112 5 10 7 97 111 9 101
a=rtpmap:0 PCMU/8000
a=rtpmap:3 GSM/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:112 AAL2-G726-32/8000
a=rtpmap:5 DVI4/8000
a=rtpmap:10 L16/8000
a=rtpmap:7 LPC/8000
a=rtpmap:97 iLBC/8000
a=fmtp:97 mode=30
a=rtpmap:111 G726-32/8000
a=rtpmap:9 G722/16000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-16
a=silenceSupp:off - - - -
a=ptime:20
a=sendrecv

---
[Jan 28 20:07:04] WARNING[20907]: chan_sip.c:2709 retrans_pkt: Maximum retries exceeded on transmission 658dc85e10e23e850022bdea3c26e16f@71.230.52.141 for seqno 102 (Non-critical Request)
[Jan 28 20:07:04] WARNING[20907]: chan_sip.c:2709 retrans_pkt: Maximum retries exceeded on transmission 422c67ab5df6bb3a1b66afdb6f53d17c@71.230.52.141 for seqno 102 (Non-critical Request)
[Jan 28 20:07:04] WARNING[20907]: chan_sip.c:2709 retrans_pkt: Maximum retries exceeded on transmission 1cdc50fc3e7a57a763fee2c464a6b67f@71.230.52.141 for seqno 102 (Non-critical Request)
Retransmitting #3 (NAT) to 68.39.201.62:32958:
INVITE sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Contact: <sip:0000000000600@71.230.52.141:5066>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 INVITE
User-Agent: matrix.gs asterisk
Date: Tue, 29 Jan 2008 01:07:01 GMT
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces, timer
Content-Type: application/sdp
Content-Length: 506

v=0
o=root 520646963 520646963 IN IP4 71.230.52.141
s=session
c=IN IP4 71.230.52.141
t=0 0
m=audio 40072 RTP/AVP 0 3 8 112 5 10 7 97 111 9 101
a=rtpmap:0 PCMU/8000
a=rtpmap:3 GSM/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:112 AAL2-G726-32/8000
a=rtpmap:5 DVI4/8000
a=rtpmap:10 L16/8000
a=rtpmap:7 LPC/8000
a=rtpmap:97 iLBC/8000
a=fmtp:97 mode=30
a=rtpmap:111 G726-32/8000
a=rtpmap:9 G722/16000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-16
a=silenceSupp:off - - - -
a=ptime:20
a=sendrecv

---
Retransmitting #4 (NAT) to 68.39.201.62:32958:
INVITE sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Contact: <sip:0000000000600@71.230.52.141:5066>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 INVITE
User-Agent: matrix.gs asterisk
Date: Tue, 29 Jan 2008 01:07:01 GMT
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces, timer
Content-Type: application/sdp
Content-Length: 506

v=0
o=root 520646963 520646963 IN IP4 71.230.52.141
s=session
c=IN IP4 71.230.52.141
t=0 0
m=audio 40072 RTP/AVP 0 3 8 112 5 10 7 97 111 9 101
a=rtpmap:0 PCMU/8000
a=rtpmap:3 GSM/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:112 AAL2-G726-32/8000
a=rtpmap:5 DVI4/8000
a=rtpmap:10 L16/8000
a=rtpmap:7 LPC/8000
a=rtpmap:97 iLBC/8000
a=fmtp:97 mode=30
a=rtpmap:111 G726-32/8000
a=rtpmap:9 G722/16000
a=rtpmap:101 telephone-event/8000
a=fmtp:101 0-16
a=silenceSupp:off - - - -
a=ptime:20
a=sendrecv

---
Reliably Transmitting (NAT) to 68.39.201.62:32958:
CANCEL sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 CANCEL
User-Agent: matrix.gs asterisk
Content-Length: 0

---
Scheduling destruction of SIP dialog '5fad7f032dce23e1656cc688364da5f3@71.230.52.141' in 32000 ms (Method: INVITE)
  == Spawn extension (userauth, 602, 1) exited non-zero on 'IAX2/iaxy-5'
    -- Hungup 'IAX2/iaxy-5'
Retransmitting #1 (NAT) to 68.39.201.62:32958:
CANCEL sip:tyril@10.0.1.2:5061;transport=udp SIP/2.0
Via: SIP/2.0/UDP 71.230.52.141:5060;branch=z9hG4bK08baf443;rport
Max-Forwards: 70
From: "Cordless" <sip:0000000000600@71.230.52.141:5066>;tag=as0904af8b
To: <sip:tyril@10.0.1.2:5061;transport=udp>
Call-ID: 5fad7f032dce23e1656cc688364da5f3@71.230.52.141
CSeq: 102 CANCEL
User-Agent: matrix.gs asterisk
Content-Length: 0