== Using SIP RTP CoS mark 5
    -- Executing [9727579794@from-internal:1] Goto("SIP/999-0000003c", "dial-out-999,9727579794,1") in new stack
    -- Goto (dial-out-999,9727579794,1)
    -- Executing [9727579794@dial-out-999:1] Set("SIP/999-0000003c", "temp=19727579794") in new stack
    -- Executing [9727579794@dial-out-999:2] Goto("SIP/999-0000003c", "_1XXXXXX.,modified") in new stack
    -- Goto (dial-out-999,_1XXXXXX.,2)
    -- Executing [_1XXXXXX.@dial-out-999:2] GotoIf("SIP/999-0000003c", "0?keepDir") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:3] Set("SIP/999-0000003c", "CDR(cdr_direction)=2") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:4] Set("SIP/999-0000003c", "CDR(cdr_outbound_dialed_phonenumber)=19727579794") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:5] Set("SIP/999-0000003c", "CDR(cdr_outbound_from_extension)=999") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:6] Set("SIP/999-0000003c", "CDR(cdr_application)=Outbound Dial") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:7] Set("SIP/999-0000003c", "CALLERID(all)="" <2178976600>") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:8] Set("SIP/999-0000003c", "CDR(cdr_outbound_did)=2178976600") in new stack
    -- Executing [_1XXXXXX.@dial-out-999:9] Dial("SIP/999-0000003c", "SIP/flowroute/19727579794") in new stack
  == Using SIP RTP CoS mark 5
    -- Called SIP/flowroute/19727579794
       > 0x7fe604009560 -- Probation passed - setting RTP source address to 74.120.95.199:24982
       > 0x7fe604009560 -- Probation passed - setting RTP source address to 74.120.95.199:24982
    -- SIP/flowroute-0000003d is making progress passing it to SIP/999-0000003c
       > 0x7fe604009560 -- Probation passed - setting RTP source address to 74.120.95.199:24982
       > 0x7fe57457a640 -- Probation passed - setting RTP source address to 72.190.32.250:5008
       > 0x7fe57457a640 -- Probation passed - setting RTP source address to 72.190.32.250:5008
    -- SIP/flowroute-0000003d is ringing
    -- SIP/flowroute-0000003d is making progress passing it to SIP/999-0000003c
    -- SIP/flowroute-0000003d answered SIP/999-0000003c
    -- Channel SIP/flowroute-0000003d joined 'simple_bridge' basic-bridge <e41827d2-7f3a-4b94-b89e-aedc30b5a550>
    -- Channel SIP/999-0000003c joined 'simple_bridge' basic-bridge <e41827d2-7f3a-4b94-b89e-aedc30b5a550>
       > Bridge e41827d2-7f3a-4b94-b89e-aedc30b5a550: switching from simple_bridge technology to native_rtp
       > Locally RTP bridged 'SIP/999-0000003c' and 'SIP/flowroute-0000003d' in stack
       > Locally RTP bridged 'SIP/999-0000003c' and 'SIP/flowroute-0000003d' in stack
vpbx22*CLI> core show channels
Channel              Location             State   Application(Data)             
SIP/502-00000036     103@from-internal:18 Up      Dial(SIP/103&SIP/203&SIP/303,2
SIP/999-0000003c     _1XXXXXX.@dial-out-9 Up      Dial(SIP/flowroute/19727579794
SIP/flowroute-000000 (None)               Up      AppDial((Outgoing Line))      
SIP/103-00000037     (None)               Up      AppDial((Outgoing Line))      
4 active channels
2 active calls
20 calls processed
vpbx22*CLI> core show channel SIP/999-0000003c
 -- General --
           Name: SIP/999-0000003c
           Type: SIP
       UniqueID: 1476732433.316
       LinkedID: 1476732433.316
      Caller ID: 2178976600
 Caller ID Name: (N/A)
Connected Line ID: (N/A)
Connected Line ID Name: (N/A)
Eff. Connected Line ID: (N/A)
Eff. Connected Line ID Name: (N/A)
    DNID Digits: 9727579794
       Language: en
          State: Up (6)
  NativeFormats: (opus)
    WriteFormat: slin48
     ReadFormat: slin48
 WriteTranscode: Yes (slin@48000)->(opus@48000)
  ReadTranscode: Yes (opus@48000)->(slin@48000)
 Time to Hangup: 0
   Elapsed Time: 0h0m25s
      Bridge ID: e41827d2-7f3a-4b94-b89e-aedc30b5a550
 --   PBX   --
        Context: dial-out-999
      Extension: _1XXXXXX.
       Priority: 9
     Call Group: 0
   Pickup Group: 0
    Application: Dial
           Data: SIP/flowroute/19727579794
 Call Identifer: [C-0000001d]
      Variables:
BRIDGEPVTCALLID=146c809956a98cdf30e5541b4eb1e8e9@206.126.62.132:5060
BRIDGEPEER=SIP/flowroute-0000003d
DIALEDPEERNUMBER=flowroute/19727579794
DIALEDPEERNAME=SIP/flowroute-0000003d
DIALSTATUS=ANSWER
DIALEDTIME=
ANSWEREDTIME=
temp=19727579794
SIPCALLID=689821758-45226-36@BJC.BGI.B.G
SIPDOMAIN=vpbx22.primevox.net
SIPURI=sip:999@192.168.1.6:45226
  CDR Variables:
level 1: calledsubaddr=
level 1: callingsubaddr=
level 1: dnid=9727579794
level 1: cdr_outbound_did=2178976600
level 1: cdr_application=Outbound Dial
level 1: cdr_outbound_from_extension=999
level 1: cdr_outbound_dialed_phonenumber=19727579794
level 1: cdr_direction=2
level 1: clid="" <2178976600>
level 1: src=2178976600
level 1: dst=_1XXXXXX.
level 1: dcontext=dial-out-999
level 1: channel=SIP/999-0000003c
level 1: dstchannel=SIP/flowroute-0000003d
level 1: lastapp=Dial
level 1: lastdata=SIP/flowroute/19727579794
level 1: start=1476732433.052589
level 1: answer=1476732438.355837
level 1: end=0.000000
level 1: duration=25
level 1: billsec=20
level 1: disposition=8
level 1: amaflags=3
level 1: uniqueid=1476732433.316
level 1: linkedid=1476732433.316
level 1: sequence=158

vpbx22*CLI> core show channel SIP/flowroute-0000003d
 -- General --
           Name: SIP/flowroute-0000003d
           Type: SIP
       UniqueID: 1476732433.317
       LinkedID: 1476732433.316
      Caller ID: _1XXXXXX.
 Caller ID Name: (N/A)
Connected Line ID: 2178976600
Connected Line ID Name: (N/A)
Eff. Connected Line ID: 2178976600
Eff. Connected Line ID Name: (N/A)
    DNID Digits: (N/A)
       Language: en
          State: Up (6)
  NativeFormats: (ulaw)
    WriteFormat: slin48
     ReadFormat: slin48
 WriteTranscode: Yes (slin@48000)->(slin@8000)->(ulaw@8000)
  ReadTranscode: Yes (ulaw@8000)->(slin@8000)->(slin@48000)
 Time to Hangup: 0
   Elapsed Time: 0h0m34s
      Bridge ID: e41827d2-7f3a-4b94-b89e-aedc30b5a550
 --   PBX   --
        Context: from-trunk
      Extension: 
       Priority: 1
     Call Group: 0
   Pickup Group: 0
    Application: AppDial
           Data: (Outgoing Line)
 Call Identifer: [C-0000001d]
      Variables:
BRIDGEPVTCALLID=689821758-45226-36@BJC.BGI.B.G
BRIDGEPEER=SIP/999-0000003c
DIALEDPEERNUMBER=flowroute/19727579794
SIPCALLID=146c809956a98cdf30e5541b4eb1e8e9@206.126.62.132:5060
  CDR Variables:
level 1: calledsubaddr=
level 1: callingsubaddr=
level 1: dnid=
level 1: clid="" <_1XXXXXX.>
level 1: src=_1XXXXXX.
level 1: dcontext=from-trunk
level 1: channel=SIP/flowroute-0000003d
level 1: lastapp=AppDial
level 1: lastdata=(Outgoing Line)
level 1: start=1476732433.053455
level 1: answer=1476732438.355816
level 1: end=1476732438.356249
level 1: duration=5
level 1: billsec=0
level 1: disposition=8
level 1: amaflags=3
level 1: uniqueid=1476732433.317
level 1: linkedid=1476732433.316
level 1: sequence=159

    -- Channel SIP/999-0000003c left 'native_rtp' basic-bridge <e41827d2-7f3a-4b94-b89e-aedc30b5a550>
    -- Channel SIP/flowroute-0000003d left 'native_rtp' basic-bridge <e41827d2-7f3a-4b94-b89e-aedc30b5a550>