proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
INVITE sip:17022781091@204.13.235.3 SIP/2.0
Max-Forwards: 69
Session-Expires: 3600;Refresher=uac
Supported: timer
To: <sip:17022781091@84.233.240.166:5060>
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 1 INVITE
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Content-Length: 245

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 8 0 100
a=rtpmap:8 PCMA/8000
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: INVITE sip:17022781091@204.13.235.3 SIP/2.0 (43)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Max-Forwards: 69 (16)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: Session-Expires: 3600;Refresher=uac (35)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Supported: timer (16)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: To: <sip:17022781091@84.233.240.166:5060> (41)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (69)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: CSeq: 1 INVITE (14)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f (75)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 10: Content-Type: application/sdp (29)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 11: Content-Length: 245 (19)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 12:  (0)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 8 0 100 (29)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:8 PCMA/8000 (20)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (12 headers 12 lines)---
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - INVITE (With RTP)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:14056 handle_request: **** Received INVITE (5) - Command in SIP INVITE
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:1623 parse_sip_options: Begin: parsing SIP "Supported: timer"
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:1631 parse_sip_options: Found SIP option: -timer-
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:1637 parse_sip_options: Matched SIP option: timer
Sending to 84.233.237.11 : 5060 (no NAT)
Using INVITE request as basis request - 3056084-3367189779-653773@nyc001nex1.interoute.com
Found peer '84X233X237X11'
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:8796 check_user_full: Setting NAT on RTP to Off
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:8804 check_user_full: Setting NAT on UDPTL to Off
Found RTP audio format 8
Found RTP audio format 0
Found RTP audio format 100
Peer audio RTP is at port 84.233.237.3:29930
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4696 process_sdp: Peer doesn't provide T.38 UDPTL
Found description format PCMA for ID 8
Found description format PCMU for ID 0
Found description format telephone-event for ID 100
Got unsupported a:fmtp in SDP offer 
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4875 process_sdp: T38 state changed to 0 on channel <none>
Capabilities: us - 0x3f0fff (g723|gsm|ulaw|alaw|g726|adpcm|slin|lpc10|g729|speex|ilbc|g726aal2|jpeg|png|h261|h263|h263p|h264), peer - audio=0xc (ulaw|alaw)/video=0x0 (nothing), combined - 0xc (ulaw|alaw)
Non-codec capabilities (dtmf): us - 0x1 (telephone-event), peer - 0x1 (telephone-event), combined - 0x1 (telephone-event)
Peer audio RTP is at port 84.233.237.3:29930
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4945 process_sdp: We're settling with these formats: 0xc (ulaw|alaw)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:12863 handle_request_invite: Checking SIP call limits for device 
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:2886 update_call_counter: Updating call counter for incoming call
Looking for 17022781091 in bvxcanada (domain 204.13.235.3)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:3652 sip_new: *** Our native formats are 0x4 (ulaw) 
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:3653 sip_new: *** Joint capabilities are 0xc (ulaw|alaw) 
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:3654 sip_new: *** Our capabilities are 0x3f0fff (g723|gsm|ulaw|alaw|g726|adpcm|slin|lpc10|g729|speex|ilbc|g726aal2|jpeg|png|h261|h263|h263p|h264) 
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:3655 sip_new: *** AST_CODEC_CHOOSE formats are 0x4 (ulaw) 
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:3678 sip_new: This channel will not be able to handle video.
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:7622 build_route: build_route: Contact hop: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
list_route: hop: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:12934 handle_request_invite: SIP/4000-081d6ca8: New call is still down.... Trying... 
Transmitting (no NAT) to 84.233.237.11:5060:
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f;received=84.233.237.11
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 1 INVITE
User-Agent: VC
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Contact: <sip:17022781091@204.13.235.3>
Content-Length: 0

---
[Sep 13 20:35:50] DEBUG[20383]: devicestate.c:303 __ast_device_state_changed_literal: Notification of state change to be queued on device/channel SIP/4000-081d6ca8
[Sep 13 20:35:50] DEBUG[20381]: devicestate.c:161 ast_device_state: No provider found, checking channel drivers for SIP - 4000
[Sep 13 20:35:50] DEBUG[20381]: chan_sip.c:14643 sip_devicestate: Checking device state for peer 4000
[Sep 13 20:35:50] DEBUG[20381]: devicestate.c:287 do_state_change: Changing state for SIP/4000 - state 4 (Invalid)
[Sep 13 20:35:50] DEBUG[21136]: pbx.c:1684 pbx_extension_helper: Launching 'Goto'
    -- Executing [17022781091@bvxcanada:1] Goto("SIP/4000-081d6ca8", "newoutboundcp|7022781091|1") in new stack
    -- Goto (newoutboundcp,7022781091,1)
[Sep 13 20:35:50] DEBUG[21136]: pbx.c:1684 pbx_extension_helper: Launching 'Dial'
    -- Executing [7022781091@newoutboundcp:1] Dial("SIP/4000-081d6ca8", "SIP/017022781091@204.13.233.252") in new stack
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:14701 sip_request_call: Asked to create a SIP channel with formats: 0x4 (ulaw)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for (No Call-ID) - INVITE (With RTP)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:3652 sip_new: *** Our native formats are 0x4 (ulaw) 
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:3653 sip_new: *** Joint capabilities are 0x0 (nothing) 
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:3654 sip_new: *** Our capabilities are 0x104 (ulaw|g729) 
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:3655 sip_new: *** AST_CODEC_CHOOSE formats are 0x4 (ulaw) 
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:3657 sip_new: *** Our preferred formats from the incoming channel are 0x4 (ulaw) 
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:3678 sip_new: This channel will not be able to handle video.
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:16203 sip_set_rtp_peer: Early remote bridge setting SIP '7dfdcbc376422b3f544681220d49a019@204.13.235.3' - Sending media to 84.233.237.3
[Sep 13 20:35:50] DEBUG[21136]: rtp.c:1511 ast_rtp_make_compatible: Seeded SDP of 'SIP/204.13.233.252-08232200' with that of 'SIP/4000-081d6ca8'
[Sep 13 20:35:50] DEBUG[21136]: channel.c:3103 ast_channel_inherit_variables: Not copying variable STACK-newoutboundcp-7022781091-1.
[Sep 13 20:35:50] DEBUG[21136]: channel.c:3103 ast_channel_inherit_variables: Not copying variable STACK-bvxcanada-17022781091-1.
[Sep 13 20:35:50] DEBUG[21136]: channel.c:3103 ast_channel_inherit_variables: Not copying variable SIPCALLID.
[Sep 13 20:35:50] DEBUG[21136]: channel.c:3103 ast_channel_inherit_variables: Not copying variable SIPDOMAIN.
[Sep 13 20:35:50] DEBUG[21136]: channel.c:3103 ast_channel_inherit_variables: Not copying variable SIPURI.
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:2726 sip_call: Outgoing Call for 017022781091
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:2886 update_call_counter: Updating call counter for outgoing call
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:2734 sip_call: Our T38 capability (3840), joint T38 capability (3840)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:5844 add_sdp: ** Our capability: 0x104 (ulaw|g729) Video flag: False
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:5845 add_sdp: ** Our prefcodec: 0x4 (ulaw) 
Audio is at 204.13.235.3 port 11258
Adding codec 0x4 (ulaw) to SDP
Adding codec 0x100 (g729) to SDP
Adding non-codec 0x1 (telephone-event) to SDP
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:5997 add_sdp: -- Done with adding codecs to SDP
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:6036 add_sdp: Done building SDP. Settling with this capability: 0x104 (ulaw|g729)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 0: INVITE sip:017022781091@204.13.233.252 SIP/2.0 (45)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport (63)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 2: From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae (63)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 3: To: <sip:017022781091@204.13.233.252> (36)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 4: Contact: <sip:9739999100@204.13.235.3> (38)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 5: Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3 (54)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 6: CSeq: 102 INVITE (16)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 7: User-Agent: VC (14)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 8: Max-Forwards: 70 (16)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 9: Date: Thu, 14 Sep 2006 01:35:50 GMT (35)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 10: Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY (66)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 11: Supported: replaces (19)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 12: Content-Type: application/sdp (29)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 13: Content-Length: 275 (19)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 14:  (0)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: o=root 20377 20377 IN IP4 84.233.237.3 (38)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: s=session (9)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 18 100 (30)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=rtpmap:18 G729/8000 (21)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=fmtp:18 annexb=no (19)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-16 (15)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=silenceSupp:off - - - - (25)
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
Reliably Transmitting (no NAT) to 204.13.233.252:5060:
INVITE sip:017022781091@204.13.233.252 SIP/2.0
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport
From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
To: <sip:017022781091@204.13.233.252>
Contact: <sip:9739999100@204.13.235.3>
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 102 INVITE
User-Agent: VC
Max-Forwards: 70
Date: Thu, 14 Sep 2006 01:35:50 GMT
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Content-Type: application/sdp
Content-Length: 275

v=0
o=root 20377 20377 IN IP4 84.233.237.3
s=session
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 18 100
a=rtpmap:0 PCMU/8000
a=rtpmap:18 G729/8000
a=fmtp:18 annexb=no
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-16
a=silenceSupp:off - - - -
a=sendrecv

---
[Sep 13 20:35:50] DEBUG[21136]: chan_sip.c:1914 __sip_reliable_xmit: *** SIP TIMER: Initalizing retransmit timer on packet: Id  #1864
    -- Called 017022781091@204.13.233.252
[Sep 13 20:35:50] DEBUG[21137]: app_queue.c:535 changethread: Device 'SIP/4000' changed to state '4' (Invalid) but we don't care because they're not a member of any queue.
proxy1*CLI> 
<-- SIP read from 204.13.233.252:5060: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport
To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc
From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 102 INVITE
Server: Lucent-Universal-Gateway
User-Agent: Lucent-Universal-Gateway
Content-Length: 0

[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 100 Trying (18)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport (63)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc (67)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae (63)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3 (54)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 102 INVITE (16)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Server: Lucent-Universal-Gateway (32)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: User-Agent: Lucent-Universal-Gateway (36)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 0 (17)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
--- (9 headers 0 lines)---
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:2055 __sip_semi_ack: *** SIP TIMER: Cancelling retransmission #1864 - INVITE (got response)
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:2064 __sip_semi_ack: (Provisional) Stopping retransmission (but retaining packet) on '7dfdcbc376422b3f544681220d49a019@204.13.235.3' Request 102: Found
[Sep 13 20:35:50] DEBUG[20383]: chan_sip.c:11212 handle_response_invite: SIP response 100 to standard invite
proxy1*CLI> 
                 
proxy1*CLI> 
<-- SIP read from 204.13.233.252:5060: 
SIP/2.0 183 Session Progress
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport
To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc
From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 102 INVITE
Contact: <sip:7022781091@204.13.233.252:5060;user=phone>
Content-Type: application/sdp
Server: Lucent-Universal-Gateway
User-Agent: Lucent-Universal-Gateway
Content-Length: 235

v=0
o=APX1 527030208 527030208 IN IP4 204.13.233.252
s=Session SDP
c=IN IP4 204.13.233.252
t=0 0
m=audio 46756 RTP/AVP 0 100
a=silenceSupp:off
a=ecan:b on g168
a=ptime:20
a=rtpmap:100 telephone-event/8000
a=rtpmap:0 PCMU/8000

[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 183 Session Progress (28)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport (63)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc (67)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae (63)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3 (54)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 102 INVITE (16)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Contact: <sip:7022781091@204.13.233.252:5060;user=phone> (55)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Content-Type: application/sdp (29)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Server: Lucent-Universal-Gateway (32)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9: User-Agent: Lucent-Universal-Gateway (36)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 10: Content-Length: 235 (19)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 11:  (0)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=APX1 527030208 527030208 IN IP4 204.13.233.252 (47)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=Session SDP (13)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 204.13.233.252 (22)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 46756 RTP/AVP 0 100 (27)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=silenceSupp:off (17)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=ecan:b on g168 (16)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=ptime:20 (10)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
--- (11 headers 11 lines)---
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:2064 __sip_semi_ack: (Provisional) Stopping retransmission (but retaining packet) on '7dfdcbc376422b3f544681220d49a019@204.13.235.3' Request 102: Found
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:11212 handle_response_invite: SIP response 183 to standard invite
Found RTP audio format 0
Found RTP audio format 100
Peer audio RTP is at port 204.13.233.252:46756
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4696 process_sdp: Peer doesn't provide T.38 UDPTL
Got unsupported a:ptime in SDP offer 
Found description format telephone-event for ID 100
Found description format PCMU for ID 0
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4875 process_sdp: T38 state changed to 0 on channel SIP/204.13.233.252-08232200
Capabilities: us - 0x104 (ulaw|g729), peer - audio=0x4 (ulaw)/video=0x0 (nothing), combined - 0x4 (ulaw)
Non-codec capabilities (dtmf): us - 0x1 (telephone-event), peer - 0x1 (telephone-event), combined - 0x1 (telephone-event)
Peer audio RTP is at port 204.13.233.252:46756
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4945 process_sdp: We're settling with these formats: 0x4 (ulaw)
[Sep 13 20:35:54] DEBUG[20383]: chan_sip.c:4952 process_sdp: We have an owner, now see if we need to change this call
    -- SIP/204.13.233.252-08232200 is making progress passing it to SIP/4000-081d6ca8
[Sep 13 20:35:54] DEBUG[21136]: chan_sip.c:16203 sip_set_rtp_peer: Early remote bridge setting SIP '3056084-3367189779-653773@nyc001nex1.interoute.com' - Sending media to 204.13.233.252
[Sep 13 20:35:54] DEBUG[21136]: rtp.c:1446 ast_rtp_early_bridge: Setting early bridge SDP of 'SIP/4000-081d6ca8' with that of 'SIP/204.13.233.252-08232200'
[Sep 13 20:35:54] DEBUG[21136]: chan_sip.c:5844 add_sdp: ** Our capability: 0xc (ulaw|alaw) Video flag: True
[Sep 13 20:35:54] DEBUG[21136]: chan_sip.c:5845 add_sdp: ** Our prefcodec: 0x0 (nothing) 
Audio is at 204.13.235.3 port 12242
Adding codec 0x4 (ulaw) to SDP
Adding codec 0x8 (alaw) to SDP
Adding non-codec 0x1 (telephone-event) to SDP
[Sep 13 20:35:54] DEBUG[21136]: chan_sip.c:5997 add_sdp: -- Done with adding codecs to SDP
[Sep 13 20:35:54] DEBUG[21136]: chan_sip.c:6036 add_sdp: Done building SDP. Settling with this capability: 0xc (ulaw|alaw)
Transmitting (no NAT) to 84.233.237.11:5060:
SIP/2.0 183 Session Progress
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f;received=84.233.237.11
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 1 INVITE
User-Agent: VC
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Contact: <sip:17022781091@204.13.235.3>
Content-Type: application/sdp
Content-Length: 254

v=0
o=root 20377 20377 IN IP4 204.13.233.252
s=session
c=IN IP4 204.13.233.252
t=0 0
m=audio 46756 RTP/AVP 0 8 100
a=rtpmap:0 PCMU/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-16
a=silenceSupp:off - - - -
a=sendrecv

---
proxy1*CLI> 
<-- SIP read from 204.13.233.252:5060: 
SIP/2.0 200 OK
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport
To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc
From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 102 INVITE
Contact: <sip:7022781091@204.13.233.252:5060;user=phone>
Accept: application/sdp
Accept-Encoding: 
Accept-Language: en
Content-Type: application/sdp
Server: Lucent-Universal-Gateway
User-Agent: Lucent-Universal-Gateway
Content-Length: 235

v=0
o=APX1 527030208 527030208 IN IP4 204.13.233.252
s=Session SDP
c=IN IP4 204.13.233.252
t=0 0
m=audio 46756 RTP/AVP 0 100
a=silenceSupp:off
a=ecan:b on g168
a=ptime:20
a=rtpmap:100 telephone-event/8000
a=rtpmap:0 PCMU/8000

[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK15a711c0;rport (63)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc (67)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae (63)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3 (54)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 102 INVITE (16)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Contact: <sip:7022781091@204.13.233.252:5060;user=phone> (55)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Accept: application/sdp (23)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Accept-Encoding:  (17)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9: Accept-Language: en (19)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 10: Content-Type: application/sdp (29)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 11: Server: Lucent-Universal-Gateway (32)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 12: User-Agent: Lucent-Universal-Gateway (36)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 13: Content-Length: 235 (19)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 14:  (0)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=APX1 527030208 527030208 IN IP4 204.13.233.252 (47)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=Session SDP (13)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 204.13.233.252 (22)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 46756 RTP/AVP 0 100 (27)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=silenceSupp:off (17)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=ecan:b on g168 (16)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=ptime:20 (10)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
--- (14 headers 11 lines)---
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2004 __sip_ack: Acked pending invite 102
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2022 __sip_ack: Stopping retransmission on '7dfdcbc376422b3f544681220d49a019@204.13.235.3' of Request 102: Match Not Found
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:11212 handle_response_invite: SIP response 200 to standard invite
Found RTP audio format 0
Found RTP audio format 100
Peer audio RTP is at port 204.13.233.252:46756
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4696 process_sdp: Peer doesn't provide T.38 UDPTL
Got unsupported a:ptime in SDP offer 
Found description format telephone-event for ID 100
Found description format PCMU for ID 0
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4875 process_sdp: T38 state changed to 0 on channel SIP/204.13.233.252-08232200
Capabilities: us - 0x104 (ulaw|g729), peer - audio=0x4 (ulaw)/video=0x0 (nothing), combined - 0x4 (ulaw)
Non-codec capabilities (dtmf): us - 0x1 (telephone-event), peer - 0x1 (telephone-event), combined - 0x1 (telephone-event)
Peer audio RTP is at port 204.13.233.252:46756
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4945 process_sdp: We're settling with these formats: 0x4 (ulaw)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4952 process_sdp: We have an owner, now see if we need to change this call
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2886 update_call_counter: Updating call counter for outgoing call
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:7622 build_route: build_route: Contact hop: <sip:7022781091@204.13.233.252:5060;user=phone>
list_route: hop: <sip:7022781091@204.13.233.252:5060;user=phone>
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:5376 reqprep: Strict routing enforced for session 7dfdcbc376422b3f544681220d49a019@204.13.235.3
set_destination: Parsing <sip:7022781091@204.13.233.252:5060;user=phone> for address/port to send to
set_destination: set destination to 204.13.233.252, port 5060
Transmitting (no NAT) to 204.13.233.252:5060:
ACK sip:7022781091@204.13.233.252:5060;user=phone SIP/2.0
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK2a75b1f2;rport
From: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
To: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc
Contact: <sip:9739999100@204.13.235.3>
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 102 ACK
User-Agent: VC
Max-Forwards: 70
Content-Length: 0

---
[Sep 13 20:36:00] DEBUG[21136]: devicestate.c:303 __ast_device_state_changed_literal: Notification of state change to be queued on device/channel SIP/204.13.233.252-08232200
    -- SIP/204.13.233.252-08232200 answered SIP/4000-081d6ca8
[Sep 13 20:36:00] DEBUG[21136]: rtp.c:1446 ast_rtp_early_bridge: Setting early bridge SDP of 'SIP/4000-081d6ca8' with that of 'SIP/204.13.233.252-08232200'
[Sep 13 20:36:00] DEBUG[21136]: devicestate.c:303 __ast_device_state_changed_literal: Notification of state change to be queued on device/channel SIP/4000-081d6ca8
[Sep 13 20:36:00] DEBUG[21136]: chan_sip.c:3334 sip_answer: SIP answering channel: SIP/4000-081d6ca8
[Sep 13 20:36:00] DEBUG[21136]: chan_sip.c:5844 add_sdp: ** Our capability: 0xc (ulaw|alaw) Video flag: True
[Sep 13 20:36:00] DEBUG[21136]: chan_sip.c:5845 add_sdp: ** Our prefcodec: 0x0 (nothing) 
Audio is at 204.13.235.3 port 12242
Adding codec 0x4 (ulaw) to SDP
Adding codec 0x8 (alaw) to SDP
Adding non-codec 0x1 (telephone-event) to SDP
[Sep 13 20:36:00] DEBUG[21136]: chan_sip.c:5997 add_sdp: -- Done with adding codecs to SDP
[Sep 13 20:36:00] DEBUG[21136]: chan_sip.c:6036 add_sdp: Done building SDP. Settling with this capability: 0xc (ulaw|alaw)
Reliably Transmitting (no NAT) to 84.233.237.11:5060:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f;received=84.233.237.11
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 1 INVITE
User-Agent: VC
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Contact: <sip:17022781091@204.13.235.3>
Content-Type: application/sdp
Content-Length: 254

v=0
o=root 20377 20378 IN IP4 204.13.233.252
s=session
c=IN IP4 204.13.233.252
t=0 0
m=audio 46756 RTP/AVP 0 8 100
a=rtpmap:0 PCMU/8000
a=rtpmap:8 PCMA/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-16
a=silenceSupp:off - - - -
a=sendrecv

---
[Sep 13 20:36:00] DEBUG[21136]: chan_sip.c:1914 __sip_reliable_xmit: *** SIP TIMER: Initalizing retransmit timer on packet: Id  #1867
    -- Native bridging SIP/4000-081d6ca8 and SIP/204.13.233.252-08232200
[Sep 13 20:36:00] DEBUG[20381]: devicestate.c:161 ast_device_state: No provider found, checking channel drivers for SIP - 204.13.233.252
[Sep 13 20:36:00] DEBUG[20381]: chan_sip.c:14643 sip_devicestate: Checking device state for peer 204.13.233.252
[Sep 13 20:36:00] DEBUG[20381]: devicestate.c:287 do_state_change: Changing state for SIP/204.13.233.252 - state 2 (In use)
[Sep 13 20:36:00] DEBUG[20381]: devicestate.c:161 ast_device_state: No provider found, checking channel drivers for SIP - 4000
[Sep 13 20:36:00] DEBUG[20381]: chan_sip.c:14643 sip_devicestate: Checking device state for peer 4000
[Sep 13 20:36:00] DEBUG[20381]: devicestate.c:287 do_state_change: Changing state for SIP/4000 - state 4 (Invalid)
[Sep 13 20:36:00] DEBUG[21138]: app_queue.c:535 changethread: Device 'SIP/204.13.233.252' changed to state '2' (In use) but we don't care because they're not a member of any queue.
[Sep 13 20:36:00] DEBUG[21139]: app_queue.c:535 changethread: Device 'SIP/4000' changed to state '4' (Invalid) but we don't care because they're not a member of any queue.
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
ACK sip:17022781091@204.13.235.3 SIP/2.0
Max-Forwards: 69
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 1 ACK
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Length: 0

[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: ACK sip:17022781091@204.13.235.3 SIP/2.0 (40)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Max-Forwards: 69 (16)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (56)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (69)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 1 ACK (11)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c7b04bfd7519d5391e9abc7466a9bd8f (75)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 0 (17)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
--- (9 headers 0 lines)---
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:14056 handle_request: **** Received ACK (6) - Command in SIP ACK
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2012 __sip_ack: ** SIP TIMER: Cancelling retransmit of packet (reply received) Retransid #1867
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2022 __sip_ack: Stopping retransmission on '3056084-3367189779-653773@nyc001nex1.interoute.com' of Response 1: Match Not Found
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
INVITE sip:17022781091@204.13.235.3 SIP/2.0
Max-Forwards: 69
Session-Expires: 3600;Refresher=uac
Supported: timer
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 2 INVITE
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=e04a897c0a8a0af7ffba6b76a7461eb4
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: INVITE sip:17022781091@204.13.235.3 SIP/2.0 (43)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Max-Forwards: 69 (16)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: Session-Expires: 3600;Refresher=uac (35)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Supported: timer (16)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (56)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (69)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: CSeq: 2 INVITE (14)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Via: SIP/2.0/UDP 84.233.237.11:5060;branch=e04a897c0a8a0af7ffba6b76a7461eb4 (75)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 10: Content-Type: application/sdp (29)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 11: Content-Length: 221 (19)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 12:  (0)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (12 headers 11 lines)---
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:14056 handle_request: **** Received INVITE (5) - Command in SIP INVITE
Sending to 84.233.237.11 : 5060 (no NAT)
Found RTP audio format 0
Found RTP audio format 100
Peer audio RTP is at port 84.233.237.3:29930
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4696 process_sdp: Peer doesn't provide T.38 UDPTL
Found description format PCMU for ID 0
Found description format telephone-event for ID 100
Got unsupported a:fmtp in SDP offer 
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4875 process_sdp: T38 state changed to 0 on channel SIP/4000-081d6ca8
Capabilities: us - 0x3f0fff (g723|gsm|ulaw|alaw|g726|adpcm|slin|lpc10|g729|speex|ilbc|g726aal2|jpeg|png|h261|h263|h263p|h264), peer - audio=0x4 (ulaw)/video=0x0 (nothing), combined - 0x4 (ulaw)
Non-codec capabilities (dtmf): us - 0x1 (telephone-event), peer - 0x1 (telephone-event), combined - 0x1 (telephone-event)
Peer audio RTP is at port 84.233.237.3:29930
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4945 process_sdp: We're settling with these formats: 0x4 (ulaw)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4952 process_sdp: We have an owner, now see if we need to change this call
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:12912 handle_request_invite: Got a SIP re-invite for call 3056084-3367189779-653773@nyc001nex1.interoute.com
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:13001 handle_request_invite: SIP/4000-081d6ca8: This call is UP.... 
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:5844 add_sdp: ** Our capability: 0x4 (ulaw) Video flag: True
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:5845 add_sdp: ** Our prefcodec: 0x0 (nothing) 
Audio is at 204.13.235.3 port 12242
Adding codec 0x4 (ulaw) to SDP
Adding non-codec 0x1 (telephone-event) to SDP
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:5997 add_sdp: -- Done with adding codecs to SDP
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:6036 add_sdp: Done building SDP. Settling with this capability: 0x4 (ulaw)
Reliably Transmitting (no NAT) to 84.233.237.11:5060:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=e04a897c0a8a0af7ffba6b76a7461eb4;received=84.233.237.11
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 2 INVITE
User-Agent: VC
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Contact: <sip:17022781091@204.13.235.3>
Content-Type: application/sdp
Content-Length: 230

v=0
o=root 20377 20379 IN IP4 204.13.233.252
s=session
c=IN IP4 204.13.233.252
t=0 0
m=audio 46756 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-16
a=silenceSupp:off - - - -
a=sendrecv

---
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:1914 __sip_reliable_xmit: *** SIP TIMER: Initalizing retransmit timer on packet: Id  #1868
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
ACK sip:17022781091@204.13.235.3 SIP/2.0
Max-Forwards: 69
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 2 ACK
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=e04a897c0a8a0af7ffba6b76a7461eb4
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Length: 0

[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: ACK sip:17022781091@204.13.235.3 SIP/2.0 (40)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Max-Forwards: 69 (16)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (56)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (69)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 2 ACK (11)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Via: SIP/2.0/UDP 84.233.237.11:5060;branch=e04a897c0a8a0af7ffba6b76a7461eb4 (75)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 0 (17)
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
--- (9 headers 0 lines)---
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:14056 handle_request: **** Received ACK (6) - Command in SIP ACK
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2012 __sip_ack: ** SIP TIMER: Cancelling retransmit of packet (reply received) Retransid #1868
[Sep 13 20:36:00] DEBUG[20383]: chan_sip.c:2022 __sip_ack: Stopping retransmission on '3056084-3367189779-653773@nyc001nex1.interoute.com' of Response 2: Match Not Found
[Sep 13 20:36:04] DEBUG[20383]: chan_sip.c:1946 __sip_autodestruct: Auto destroying SIP dialog '7262a8db2b3bfc886f405ae46a0f67cb@67.58.3.138'
[Sep 13 20:36:04] DEBUG[20383]: chan_sip.c:2992 sip_destroy: Destroying SIP dialog 7262a8db2b3bfc886f405ae46a0f67cb@67.58.3.138
Really destroying SIP dialog '7262a8db2b3bfc886f405ae46a0f67cb@67.58.3.138' Method: OPTIONS
proxy1*CLI> 
<-- SIP read from 204.13.233.252:5060: 
BYE sip:9739999100@204.13.235.3 SIP/2.0
To: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
From: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 25366028 BYE
Via: SIP/2.0/UDP 204.13.233.252:5060
Max-Forwards: 70
Accept: application/sdp
Accept-Encoding: 
Accept-Language: en
User-Agent: Lucent-Universal-Gateway
Content-Length: 0

[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: BYE sip:9739999100@204.13.235.3 SIP/2.0 (39)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae (61)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc (69)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3 (54)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 25366028 BYE (18)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Via: SIP/2.0/UDP 204.13.233.252:5060 (35)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Max-Forwards: 70 (16)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Accept: application/sdp (23)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Accept-Encoding:  (17)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9: Accept-Language: en (19)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 10: User-Agent: Lucent-Universal-Gateway (36)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 11: Content-Length: 0 (17)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 12:  (0)
--- (12 headers 0 lines)---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:14056 handle_request: **** Received BYE (8) - Command in SIP BYE
Sending to 204.13.233.252 : 5060 (no NAT)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:13661 handle_request_bye: Received bye, issuing owner hangup
.Transmitting (no NAT) to 204.13.233.252:5060:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 204.13.233.252:5060;received=204.13.233.252
From: <sip:017022781091@204.13.233.252>;tag=04fcd0a6-1f69d7c0-26e80dcc
To: "9739999100" <sip:9739999100@204.13.235.3>;tag=as707fb2ae
Call-ID: 7dfdcbc376422b3f544681220d49a019@204.13.235.3
CSeq: 25366028 BYE
User-Agent: VC
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Contact: <sip:9739999100@204.13.235.3>
Content-Length: 0

---
[Sep 13 20:36:09] DEBUG[21136]: rtp.c:2771 bridge_native_loop: Oooh, got a hangup
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:16206 sip_set_rtp_peer: Sending reinvite on SIP '3056084-3367189779-653773@nyc001nex1.interoute.com' - It's audio soon redirected to IP 204.13.235.3
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:5376 reqprep: Strict routing enforced for session 3056084-3367189779-653773@nyc001nex1.interoute.com
set_destination: Parsing <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> for address/port to send to
set_destination: set destination to 84.233.237.11, port 5060
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:5844 add_sdp: ** Our capability: 0x4 (ulaw) Video flag: True
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:5845 add_sdp: ** Our prefcodec: 0x0 (nothing) 
Audio is at 204.13.235.3 port 12242
Adding codec 0x4 (ulaw) to SDP
Adding non-codec 0x1 (telephone-event) to SDP
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:5997 add_sdp: -- Done with adding codecs to SDP
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:6036 add_sdp: Done building SDP. Settling with this capability: 0x4 (ulaw)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:1572 initialize_initreq: Initializing already initialized SIP dialog 3056084-3367189779-653773@nyc001nex1.interoute.com (presumably reinvite)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 0: INVITE sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN" SIP/2.0 (72)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 3: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 4: Contact: <sip:17022781091@204.13.235.3> (39)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 5: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 6: CSeq: 102 INVITE (16)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 7: User-Agent: VC (14)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 8: Max-Forwards: 70 (16)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 9: Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY (66)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 10: Supported: replaces (19)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 11: X-asterisk-Info: SIP re-invite (External RTP bridge) (52)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 12: Content-Type: application/sdp (29)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 13: Content-Length: 228 (19)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4377 parse_request: Header 14:  (0)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: o=root 20377 20380 IN IP4 204.13.235.3 (38)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: s=session (9)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: c=IN IP4 204.13.235.3 (21)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: m=audio 12242 RTP/AVP 0 100 (27)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-16 (15)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=silenceSupp:off - - - - (25)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
Reliably Transmitting (no NAT) to 84.233.237.11:5060:
INVITE sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN" SIP/2.0
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Contact: <sip:17022781091@204.13.235.3>
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
User-Agent: VC
Max-Forwards: 70
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
X-asterisk-Info: SIP re-invite (External RTP bridge)
Content-Type: application/sdp
Content-Length: 228

v=0
o=root 20377 20380 IN IP4 204.13.235.3
s=session
c=IN IP4 204.13.235.3
t=0 0
m=audio 12242 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-16
a=silenceSupp:off - - - -
a=sendrecv

---
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:1914 __sip_reliable_xmit: *** SIP TIMER: Initalizing retransmit timer on packet: Id  #1869
[Sep 13 20:36:09] DEBUG[21136]: channel.c:3829 ast_channel_bridge: Returning from native bridge, channels: SIP/4000-081d6ca8, SIP/204.13.233.252-08232200
[Sep 13 20:36:09] DEBUG[21136]: channel.c:1543 ast_hangup: Hanging up channel 'SIP/204.13.233.252-08232200'
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:3187 sip_hangup: Hangup call SIP/204.13.233.252-08232200, SIP callid 7dfdcbc376422b3f544681220d49a019@204.13.235.3)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:3194 sip_hangup: update_call_counter(017022781091) - decrement call limit counter on hangup
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:2886 update_call_counter: Updating call counter for outgoing call
[Sep 13 20:36:09] DEBUG[21136]: devicestate.c:303 __ast_device_state_changed_literal: Notification of state change to be queued on device/channel SIP/204.13.233.252-08232200
[Sep 13 20:36:09] DEBUG[21136]: rtp.c:1409 ast_rtp_early_bridge: Channel '<unspecified>' has no RTP, not doing anything
[Sep 13 20:36:09] DEBUG[21136]: app_dial.c:1631 dial_exec_full: Exiting with DIALSTATUS=ANSWER.
[Sep 13 20:36:09] DEBUG[21136]: pbx.c:2280 __ast_pbx_run: Spawn extension (newoutboundcp,7022781091,1) exited non-zero on 'SIP/4000-081d6ca8'
[Sep 13 20:36:09] DEBUG[20381]: devicestate.c:161 ast_device_state: No provider found, checking channel drivers for SIP - 204.13.233.252
[Sep 13 20:36:09] DEBUG[20381]: chan_sip.c:14643 sip_devicestate: Checking device state for peer 204.13.233.252
[Sep 13 20:36:09] DEBUG[20381]: devicestate.c:287 do_state_change: Changing state for SIP/204.13.233.252 - state 2 (In use)
[Sep 13 20:36:09] DEBUG[21136]: cdr_addon_mysql.c:210 mysql_log: cdr_mysql: inserting a CDR record.
[Sep 13 20:36:09] DEBUG[21136]: cdr_addon_mysql.c:226 mysql_log: cdr_mysql: SQL command as follows: INSERT INTO cdr (calldate,clid,src,dst,dcontext,channel,dstchannel,lastapp,lastdata,duration,billsec,disposition,amaflags,accountcode) VALUES ('2006-09-13 20:35:50','9739999100','9739999100','7022781091','newoutboundcp', 'SIP/4000-081d6ca8','SIP/204.13.233.252-08232200','Dial','SIP/017022781091@204.13.233.252',19,9,'ANSWERED',3,'')
[Sep 13 20:36:09] DEBUG[21140]: app_queue.c:535 changethread: Device 'SIP/204.13.233.252' changed to state '2' (In use) but we don't care because they're not a member of any queue.
[Sep 13 20:36:09] DEBUG[21136]: channel.c:1543 ast_hangup: Hanging up channel 'SIP/4000-081d6ca8'
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:3187 sip_hangup: Hangup call SIP/4000-081d6ca8, SIP callid 3056084-3367189779-653773@nyc001nex1.interoute.com)
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:3194 sip_hangup: update_call_counter() - decrement call limit counter on hangup
[Sep 13 20:36:09] DEBUG[21136]: chan_sip.c:2886 update_call_counter: Updating call counter for incoming call
Scheduling destruction of SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' in 32000 ms (Method: ACK)
[Sep 13 20:36:09] DEBUG[21136]: devicestate.c:303 __ast_device_state_changed_literal: Notification of state change to be queued on device/channel SIP/4000-081d6ca8
[Sep 13 20:36:09] DEBUG[20381]: devicestate.c:161 ast_device_state: No provider found, checking channel drivers for SIP - 4000
[Sep 13 20:36:09] DEBUG[20381]: chan_sip.c:14643 sip_devicestate: Checking device state for peer 4000
[Sep 13 20:36:09] DEBUG[20381]: devicestate.c:287 do_state_change: Changing state for SIP/4000 - state 4 (Invalid)
[Sep 13 20:36:09] DEBUG[21141]: app_queue.c:535 changethread: Device 'SIP/4000' changed to state '4' (Invalid) but we don't care because they're not a member of any queue.
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 100 Trying
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Content-Length: 0

[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 100 Trying (18)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 102 INVITE (16)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Length: 0 (17)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7:  (0)
--- (7 headers 0 lines)---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:2055 __sip_semi_ack: *** SIP TIMER: Cancelling retransmission #1869 - INVITE (got response)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:2064 __sip_semi_ack: (Provisional) Stopping retransmission (but retaining packet) on '3056084-3367189779-653773@nyc001nex1.interoute.com' Request 102: Found
SIP Response message for INCOMING dialog INVITE arrived
Really destroying SIP dialog '7dfdcbc376422b3f544681220d49a019@204.13.235.3' Method: BYE
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:2004 __sip_ack: Acked pending invite 102
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:2022 __sip_ack: Stopping retransmission on '3056084-3367189779-653773@nyc001nex1.interoute.com' of Request 102: Match Not Found
SIP Response message for INCOMING dialog INVITE arrived
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:11212 handle_response_invite: SIP response 200 to standard invite
Found RTP audio format 0
Found RTP audio format 100
Peer audio RTP is at port 84.233.237.3:29930
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4696 process_sdp: Peer doesn't provide T.38 UDPTL
Found description format PCMU for ID 0
Found description format telephone-event for ID 100
Got unsupported a:fmtp in SDP offer 
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4875 process_sdp: T38 state changed to 0 on channel <none>
Capabilities: us - 0x3f0fff (g723|gsm|ulaw|alaw|g726|adpcm|slin|lpc10|g729|speex|ilbc|g726aal2|jpeg|png|h261|h263|h263p|h264), peer - audio=0x4 (ulaw)/video=0x0 (nothing), combined - 0x4 (ulaw)
Non-codec capabilities (dtmf): us - 0x1 (telephone-event), peer - 0x1 (telephone-event), combined - 0x1 (telephone-event)
Peer audio RTP is at port 84.233.237.3:29930
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4945 process_sdp: We're settling with these formats: 0x4 (ulaw)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:5376 reqprep: Strict routing enforced for session 3056084-3367189779-653773@nyc001nex1.interoute.com
set_destination: Parsing <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> for address/port to send to
set_destination: set destination to 84.233.237.11, port 5060
Transmitting (no NAT) to 84.233.237.11:5060:
ACK sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN" SIP/2.0
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK0233a741;rport
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Contact: <sip:17022781091@204.13.235.3>
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 ACK
User-Agent: VC
Max-Forwards: 70
Content-Length: 0

---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:5376 reqprep: Strict routing enforced for session 3056084-3367189779-653773@nyc001nex1.interoute.com
set_destination: Parsing <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> for address/port to send to
set_destination: set destination to 84.233.237.11, port 5060
Reliably Transmitting (no NAT) to 84.233.237.11:5060:
BYE sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN" SIP/2.0
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK58bf820b;rport
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Contact: <sip:17022781091@204.13.235.3>
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 103 BYE
User-Agent: VC
Max-Forwards: 70
Content-Length: 0

---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:1914 __sip_reliable_xmit: *** SIP TIMER: Initalizing retransmit timer on packet: Id  #1871
Scheduling destruction of SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' in 32000 ms (Method: ACK)
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 481 Call/Transaction Does Not Exist 
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK58bf820b;rport
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 103 BYE
Content-Length: 0

[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 481 Call/Transaction Does Not Exist  (44)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK58bf820b;rport (63)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (69)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (56)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 103 BYE (13)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Length: 0 (17)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7:  (0)
--- (7 headers 0 lines)---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:2012 __sip_ack: ** SIP TIMER: Cancelling retransmit of packet (reply received) Retransid #1871
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:2022 __sip_ack: Stopping retransmission on '3056084-3367189779-653773@nyc001nex1.interoute.com' of Request 103: Match Not Found
SIP Response message for INCOMING dialog BYE arrived
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: ACK
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - SIP/2.0 (No RTP)
[Sep 13 20:36:09] DEBUG[20383]: chan_sip.c:14022 handle_request: That's odd...  Got a response on a call we dont know about. Cseq 102 Cmd SIP/2.0
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: SIP/2.0
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - SIP/2.0 (No RTP)
[Sep 13 20:36:10] DEBUG[20383]: chan_sip.c:14022 handle_request: That's odd...  Got a response on a call we dont know about. Cseq 102 Cmd SIP/2.0
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: SIP/2.0
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:1946 __sip_autodestruct: Auto destroying SIP dialog '36cf95e50ace91a121d8a73f2898abd4@207.174.202.34'
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:2992 sip_destroy: Destroying SIP dialog 36cf95e50ace91a121d8a73f2898abd4@207.174.202.34
Really destroying SIP dialog '36cf95e50ace91a121d8a73f2898abd4@207.174.202.34' Method: OPTIONS
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - SIP/2.0 (No RTP)
[Sep 13 20:36:12] DEBUG[20383]: chan_sip.c:14022 handle_request: That's odd...  Got a response on a call we dont know about. Cseq 102 Cmd SIP/2.0
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: SIP/2.0
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - SIP/2.0 (No RTP)
[Sep 13 20:36:16] DEBUG[20383]: chan_sip.c:14022 handle_request: That's odd...  Got a response on a call we dont know about. Cseq 102 Cmd SIP/2.0
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: SIP/2.0
proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - SIP/2.0 (No RTP)
[Sep 13 20:36:20] DEBUG[20383]: chan_sip.c:14022 handle_request: That's odd...  Got a response on a call we dont know about. Cseq 102 Cmd SIP/2.0
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: SIP/2.0
proxy1*CLI> 

<-- SIP read from 84.233.237.11:5060: 
SIP/2.0 200 OK
To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 102 INVITE
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Type: application/sdp
Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport
Content-Length: 221

v=0
o=nyc001nex 1234 22172 IN IP4 84.233.237.3
s=sip call
c=IN IP4 84.233.237.3
t=0 0
m=audio 29930 RTP/AVP 0 100
a=rtpmap:0 PCMU/8000
a=rtpmap:100 telephone-event/8000
a=fmtp:100 0-15
a=sendrecv
a=maxptime:20

[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: SIP/2.0 200 OK (14)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: To: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (67)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: From: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (58)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: CSeq: 102 INVITE (16)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Content-Type: application/sdp (29)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Via: SIP/2.0/UDP 204.13.235.3:5060;branch=z9hG4bK77e4992f;rport (63)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 221 (19)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: v=0 (3)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: o=nyc001nex 1234 22172 IN IP4 84.233.237.3 (42)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: s=sip call (10)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: c=IN IP4 84.233.237.3 (21)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: t=0 0 (5)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: m=audio 29930 RTP/AVP 0 100 (27)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:0 PCMU/8000 (20)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=rtpmap:100 telephone-event/8000 (33)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=fmtp:100 0-15 (15)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=sendrecv (10)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4409 parse_request: Line: a=maxptime:20 (13)
--- (9 headers 11 lines)---
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - SIP/2.0 (No RTP)
[Sep 13 20:36:24] DEBUG[20383]: chan_sip.c:14022 handle_request: That's odd...  Got a response on a call we dont know about. Cseq 102 Cmd SIP/2.0
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: SIP/2.0
proxy1*CLI> 
proxy1*CLI> sip show channels
Peer             User/ANR    Call ID      Seq (Tx/Rx)  Form  Hold     Last Message   
204.13.233.229   (None)      7270afd5234  00101/00102  unkn  No       Rx: OPTIONS               
67.58.3.154      (None)      3a0270dd3b6  00101/00102  unkn  No       Rx: OPTIONS               
204.13.233.252    0141679224  69af713c6d0  00102/00000  g729  No       Tx: ACK                   
66.219.105.44    92489       06a6e6e8187  00101/00102  g729  No       Rx: ACK                   
204.13.233.252    0121492392  77c4fca907e  00102/00000  ulaw  No       Tx: ACK                   
208.67.249.131   6141443444  630cdc034d0  00101/00102  ulaw  No       Rx: ACK                   
6 active SIP channels

(((( NO ZOMBIE CHANNEL RIGHT NOW ))))

proxy1*CLI> 
<-- SIP read from 84.233.237.11:5060: 
BYE sip:17022781091@204.13.235.3 SIP/2.0
Max-Forwards: 69
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 3 BYE
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c30c08bdef0f47a46f61158f0c936437
Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN">
Content-Length: 0

[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 0: BYE sip:17022781091@204.13.235.3 SIP/2.0 (40)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 1: Max-Forwards: 69 (16)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 2: To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4 (56)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 3: From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7 (69)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 4: Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com (59)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 5: CSeq: 3 BYE (11)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 6: Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c30c08bdef0f47a46f61158f0c936437 (75)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 7: Contact: <sip:9739999100@84.233.237.11:5060;tgrp="TTN_USSS7_TTN_IN"> (68)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 8: Content-Length: 0 (17)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4377 parse_request: Header 9:  (0)
--- (9 headers 0 lines)---
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:4157 sip_alloc: Allocating new SIP dialog for 3056084-3367189779-653773@nyc001nex1.interoute.com - BYE (No RTP)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:14056 handle_request: **** Received BYE (8) - Command in SIP BYE
Sending to 84.233.237.11 : 5060 (no NAT)
Scheduling destruction of SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' in 32000 ms (Method: BYE)
[Sep 13 20:36:30] DEBUG[20383]: chan_sip.c:13665 handle_request_bye: Received bye, no owner, selfdestruct soon.
.Transmitting (no NAT) to 84.233.237.11:5060:
SIP/2.0 200 OK
Via: SIP/2.0/UDP 84.233.237.11:5060;branch=c30c08bdef0f47a46f61158f0c936437;received=84.233.237.11
From: <sip:9739999100@84.233.237.11:4000;cpc=ordinary>;tag=gK094dd7d7
To: <sip:17022781091@84.233.240.166:5060>;tag=as5d83c1b4
Call-ID: 3056084-3367189779-653773@nyc001nex1.interoute.com
CSeq: 3 BYE
User-Agent: VC
Allow: INVITE, ACK, CANCEL, OPTIONS, BYE, REFER, SUBSCRIBE, NOTIFY
Supported: replaces
Content-Length: 0

---
proxy1*CLI> sip show channels
Peer             User/ANR    Call ID      Seq (Tx/Rx)  Form  Hold     Last Message   
84.233.237.11    (None)      3056084-336  00101/00003  unkn  No       Rx: BYE                   
204.13.233.229   (None)      7270afd5234  00101/00102  unkn  No       Rx: OPTIONS               
67.58.3.154      (None)      3a0270dd3b6  00101/00102  unkn  No       Rx: OPTIONS               
204.13.233.252    0141679224  69af713c6d0  00102/00000  g729  No       Tx: ACK                   
66.219.105.44    92489       06a6e6e8187  00101/00102  g729  No       Rx: ACK                   
204.13.233.252    0121492392  77c4fca907e  00102/00000  ulaw  No       Tx: ACK                   
208.67.249.131   6141443444  630cdc034d0  00101/00102  ulaw  No       Rx: ACK                   
7 active SIP channels

(((( NOW WE HAVE A ZOMBIE CHANNEL ))))
84.233.237.11    (None)      3056084-336  00101/00003  unkn  No       Rx: BYE  

[Sep 13 20:37:02] DEBUG[20383]: chan_sip.c:1946 __sip_autodestruct: Auto destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com'
[Sep 13 20:37:02] DEBUG[20383]: chan_sip.c:2992 sip_destroy: Destroying SIP dialog 3056084-3367189779-653773@nyc001nex1.interoute.com
Really destroying SIP dialog '3056084-3367189779-653773@nyc001nex1.interoute.com' Method: BYE